DORMA-Glas Pendeltürband MARCATO Motion

Bezeichnung: MARCATO Motion

Ausführung: Hydraulisches Pendeltürband

Hersteller: DORMA-Glas GmbH

PRODUKTBESCHREIBUNG / FUNKTIONEN

Band mit federgestützter Selbstschliessfunktion

sowie hydraulischer Dämpfung. Einstellbare Schließgeschwindigkeit.

Feststellung bei 90° Öffnungswinkel bezogen auf die Nulllage.

TECHNISCHE MERKMALE

- Material: Aluminium

- Oberflächen: Eloxaltöne

- Glasart: ESG

- Glasdicke: 8, 10, 12 mm

- Max. Flügelgewicht: 65 kg

- Max. Flügelbreite: 1000 mm

- Feuchtraum geeignet

- auch für einseitigen Anschlag geeignet

- nur für den Innenbereich, nicht geeignet für Türen im hochfrequentierten

Bereich/öffentlichen Gebäuden

EINSATZBEREICHE

1-/2-flügelige Anlagen, Anlagen mit Seitenteil

PRODUKTAUSFÜHRUNG

- Paar Pendeltürband zur seitlichen Montage an Wand

oder Zarge mit aufliegender Montageplatte '..........'

- Paar Pendeltürb. z. Montage Glas an Glas '..........'

TÜRART

Glastür

FARBE

Abhängig von Produktausführung:

- LM silber eloxiert (Silber N 600 ST) '..........'

- LM niro eloxiert (Niro N 700) '..........'

OPTIONEN

- 8 mm ESG '..........'

- 10 mm ESG '..........'

- 12 mm ESG '..........'

ZUBEHÖR

- Easy Stop f. Pendeltüren - f. 8 mm Glas '..........'

- Easy Stop f. Pendeltüren - f. 10 mm Glas '..........'

- Easy Stop f. Pendeltüren - f. 12 mm Glas '..........'

- Boden-Türstopper '..........'

- Wand-Türstopper, kurz '..........'

- Wand-Türstopper, lang '..........'

DORMA-Glas double action door hinge MARCATO Motion

Designation: MARCATO Motion

Description: Hydraulic double action door hinge

Manufacturer: DORMA-Glas GmbH

PRODUCT DESCRIPTION / FUNCTIONS

Hinge with spring supported self-closing function

and hydraulic damping. Adjustable closing speed.

Locking at 90° opening angle in relation to the zero position.

TECHNICAL FEATURES

- Material: Aluminum

- Surfaces: Anodized colors

- Glass type: TSG (Toughened safety glass)

- Glass thickness: 8, 10, 12 mm

- Max. door weight: 65 kg

- Max. door width: 1000 mm

- Suitable for humid environments

- Also suitable for single action door (with stop) applications

- For interior use only, not suitable for doors in highly frequented

area/public buildings

AREAS OF APPLICATION

1-/2-leaf systems, systems with side panel

PRODUCT VERSION

- Pair of double action door hinges for installation onto wall

or frame with surface-mounted mounting plate '............'

- Pair of double action door hinges for installation glass to glass '............'

DOOR TYPE

Glass door

COLOR

Depending on product design:

- AL silver anodised (silver N 600 ST) '..........'

- AL niro anodized (Niro N 700)'..........'

OPTIONS

- 8 mm TSG '..........'

- 10 mm TSG '...........'

- 12 mm TSG '...........'

ACCESSORIES

- Easy Stop f. double action doors - f. 8 mm glass '..........'

- Easy Stop f. double action doors - f. 10 mm glass '..........'

- Easy Stop f. double action doors - f. 12 mm glass '..........'

- Floor doorstopper '..........'

- Wall doorstop, short '..........'

- Wall doorstop, long '..........'